| SONATA(YF) >2013 > G 2.4 GDI > Engine Control/Fuel System > Engine Control System > Fuel Pressure Control Valve>Repair procedures |

Inspection

1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.

2. | Disconnect the fuel pressure regulator valve connector.

3. | Measure resistance between the fuel pressure regulator valve terminals 1 and 2.

4. | Check that the resistance is within the specification.

Specification: Refer to “Specification”