| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Audio>Specifications |

Specifications

Audio

Item | Specification
Model | RADIO/CD/MP3 (PA710S) | RADIO/CDC/MP3 (PA760S)
Power supply | DC 14.4V
Dark current | Max 2.0mA (Head unit only)
Antenna | 80PF 75Ω
Tuning type | PLL SYNTHESIZED TUNING
Frequency range | FM | 87.5~107.9 MHz / 200KHz
/ Channel space | AM | 530~1710 KHz / 10KHz

Speaker

Item | PA710S | PA760S
Input power (W or V) | Front | MAX 40W | MAX 40W
Rear | MAX 40W | MAX 40W
Midrange | MAX 30W | MAX 30W
Sub woofer | - | MAX 40W
Impedance(Ω) | Front | 4 ± 0.6 | 2 ± 0.3
Rear | 4 ± 0.6 | 2 ± 0.3
Midrange | 4 ± 0.6 | 2 ± 0.3
Sub woofer | - | 2 ± 0.3
Number of speaker | 6 | 7