| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Lighting System > Overhead Console Lamp>Repair procedures |

Inspection

Remove the overhead console lamp assembly then check for continuity between terminals. If the continuity is not as specified, replace the map lamp switch.

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Loosen 2 screws holding the overhead console (A).

3. | Disconnect the connectors (A) of sunroof switch and lamp switch then remove the overhead console lamp assembly.

4. | If necessary to replace the bulb, replace the bulb after opening the overhead console lens.

Installation

1. | Install the overhead console lamp after connecting the sunroof switch connector and lamp connector.

2. | Install the lens after tightening 2 screws.