| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Lighting System > Hazard Lamp Switch>Repair procedures |

Inspection

Hazard Lamp Switch

1. | Remove the center fascia panel. (Refer to the BD group - "Crash pad")

2. | Disconnect the switch from the center fascia panel.

3. | Operate the switch and check for continuity between terminals.

Removal

1. | Disconnect the negative(-) battery terminal.

2. | Remove the crash pad garnish. (Refer to the BD group - "Crash pad")

3. | Remove the center fascia panel (B) with hazard lamp switch (A).

4. | Disconnect the hazard lamp switch connector (A) and heater control unit connector (B).

Installation

1. | Install the hazard lamp switch.

2. | Install the center fascia panel.

3. | Install the crash pad garnish.