| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Power Windows > Power Window Switch>Repair procedures |

Inspection

Power Window Main Switch Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Remove the front door trim panel. (Refer to the BD group - "Front door")

3. | Disconnect the connector from the switch.

4. | Check for continuity between the terminals in each switch position according to the table. If the continuity condition is not normal, replace the switch. [Auto Up/Down] [Auto Down Only]

Passenger Power Window Switch Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Remove the front door trim panel. (Refer to the BD group - "Front door")

3. | Disconnect the connector from the switch.

4. | Check for continuity between the terminals in each switch position according to the table. If the continuity condition is not normal, replace the switch.

Rear Power Window Switch Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Remove the rear door trim panel. (Refer to the BD group - "Rear door")

3. | Disconnect the 8P connector from the switch.

4. | Check for continuity between the terminals in each switch position according to the table. If the continuity condition is not normal, replace the switch.