| SONATA(YF) >2012 > G 2.4 GDI > Engine Control/Fuel System > Fuel Delivery System > Accelerator Pedal>Repair procedures |

Removal

1. | Turn the ignition switch OFF and disconnect the negative (-) battery cable.

2. | Disconnect the accelerator position sensor connector (A).

3. | Remove the installation nuts (B) and bolt (C), and then remove the accelerator pedal module.

Installation

1. | Installation is reverse of removal.

Accelerator pedal module installation nut:
9.8 ~ 14.7 N.m (1.0 ~ 1.5 kgf.m, 7.2 ~ 10.8 lb-ft)
Accelerator pedal module installation bolt:
8.8 ~ 13.7 N.m (0.9 ~ 1.4 kgf.m, 6.5 ~ 10.1 lb-ft)