| SONATA(YF) >2013 > G 2.4 GDI > Engine Control/Fuel System > Engine Control System > Variable Intake Solenoid (VIS) Valve>Repair procedures |

Inspection

1. | Turn the ignition switch OFF.

2. | Disconnect the VIS valve connector.

3. | Measure resistance between VIS valve terminals 1 and 2.

Specification: Refer to "Specification"

Removal

1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.

2. | Disconnect the variable intake solenoid valve connector (A).

3. | Disconnect the vacuum hoses (B,C) from the valve.

4. | Remove the installation bolt (D), and then remove the valve from the surge tank.

Installation

• | Install the component with the specified torques.

• | Note that internal damage may occur when the component is dropped. If the component has been dropped, inspect before installing.

• | Use care to keep foreign material out of the valve.

1. | Installation is reverse of removal.