| SONATA(YF) >2013 > G 2.4 GDI > Suspension System > Tires/Wheels > Wheel>Repair procedures |

Hub nut tightening sequence

Tighten the hub nuts as follows.

Tightening torque:
88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft)

When using an impact gun, final tightening torque should be checked using a torque wrench.

Run out inspection

1. | Jack up the vehicle.

2. | Measure the wheel Run-out by using a dial indicator as illustration below.

Run-out | Aluminum
Radial mm(in.) | Below 0.3(0.012)
Lateral mm(in.) | Below 0.3(0.012)

3. | If measured value exceeds the standard value, replace the wheel.