| SONATA(YF) >2013 > G 2.4 GDI > Body (Interior and Exterior) > Interior > Console>Repair procedures |

Replacement

Floor Console Replacement

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.

• | Put on gloves to protect your hands.

1. | Using a screwdriver or remover, remove the crash pad garnish (A).

2. | Using a screwdriver, remove the knob (A) and boots (B).

3. | Using a screwdriver or remover, remove the console upper cover (A).

4. | Disconnect the connectors (A).

5. | Remove the extension side cover (A).

6. | Remove the console tray mat (A).

7. | After loosening the console mounting screws and bolts, then remove the console assembly (A).

8. | Installation is the reverse of removal.

• | Make sure all connectors are connected properly.

• | Replace any damage clips.

Armrest Replacement

1. | After loosening the mounting screws, then remove the console rear cover (A).

2. | After loosening the mounting screws, then remove the armrest (A).

3. | Installation is the reverse of removal.