| SONATA(YF) >2013 > G 2.4 GDI > Steering System > General Information>Specifications |

Specifications

Item | Specification
Type | Motor driven power steering system(EPS)
Steering gear | Type | Rack & Pinion
Rack stroke | 148mm (5.82 in.)
Steering angle(Max.) | Inner | 39.83°±1.5°
Outer | 33.01°

Tightening Torques

Item | Tightening torque
Nm | kgf.m | lb-ft
Hub nuts | 88.3 ~ 107.9 | 9.0 ~ 11.0 | 65.1 ~ 79.6
Steering wheel lock nut | 39.2 ~ 49.0 | 4.0 ~ 5.0 | 28.9 ~ 36.2
Steering column mounting bolts and nuts | 12.7 ~ 17.7 | 1.3 ~ 1.8 | 9.4 ~ 13.0
Steering column to Universal joint | 53.9 ~ 63.7 | 5.5 ~ 6.5 | 39.8 ~ 47.0
Universal joint to pinion of steering gear | 32.4 ~ 37.3 | 3.3 ~ 3.8 | 23.9 ~ 27.5
Tie rod end castle nut | 34.3 ~ 44.1 | 3.5 ~ 4.5 | 25.3 ~ 32.5
Lower arm ball joint bolts | 98.1 ~ 117.7 | 10.0 ~ 12.0 | 72.3 ~ 86.8
Steering gear box mounting bolts | 88.3 ~ 107.9 | 9.0 ~ 11.0 | 65.1 ~ 79.6
Stabilizer link nut | 98.1 ~ 117.7 | 10.0 ~ 12.0 | 72.3 ~ 86.8
Sub frame stay mounting bolts & nuts | 44.1 ~ 58.8 | 4.5 ~ 6.0 | 32.5 ~ 43.4
Sub frame mounting bolts & nuts | 156.9 ~ 176.5 | 16.0 ~ 18.0 | 115.7 ~ 130.2
Roll rod mounting bolt & nut | 107.9 ~ 127.5 | 11.0 ~13.0 | 79.6 ~ 94.0