| SONATA(YF) >2012 > G 2.4 GDI > Engine Electrical System > Starting System > Starter Relay>Repair procedures |

Inspection

1. | Remove the fuse box cover.

2. | Remove the starter relay (A).

3. | Using an ohmmeter, check that there is continuity between each terminal.

Terminal | Continuity
30 - 87 | NO
85 - 86 | YES

4. | Apply 12V to terminal 85 and ground to terminal 86. Check for continuity between terminals 30 and 87.

5. | If there is no continuity, replace the starter relay.

6. | Install the starter relay.

7. | Install the fuse box cover.