| SONATA(YF) >2012 > G 2.4 GDI > Engine Control/Fuel System > Engine Control System > Heated Oxygen Sensor (HO2S)>Specifications |

Specification

HO2S [Bank 1/Sensor 1]

Item | Specification
Heater Resistance (Ω) | 2.5 ~ 4.0 [20°C(68°F)]

HO2S [Bank 1/Sensor 2]

A/F Ratio (λ) | Output Voltage(V)
RICH | Approx. 0.9
LEAN | Approx. 0.04

Item | Specification
Heater Resistance (Ω) | 3.3 ~ 4.1Ω[21°C(69.8°F)]