| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Immobilizer System > Immobilizer Control Unit>Repair procedures |

Replacement

1. | Disconnect the negative (-) battery terminal.

2. | Remove the crash pad lower panel. (Refer to the BD group - "Crash pad")

3. | Disconnect the 5P connector of the SMARTRA unit and then remove the SMARTRA unit (A) after loosening the bolt.

4. | Installation is the reverse of removal procedure.