| SONATA(YF) >2012 > G 2.4 GDI > Heating,Ventilation, Air Conditioning > General Information>Specifications |

Specification

Air Conditioner

Item | Specification
Compressor | Type | 6VSX16
Oil type & Capacity | PAG OIL 150±10
Pulley type | 6PK-TYPE
Displacement | 160cc/rev
Condenser | Heat rejection | 14,000 ±5% kcal/hr
A/C Pressure transducer | The method to measure the pressure | Voltage= 0.00878835 * Pressure (psig) + 0.5
Expansion valve | Type | Block type
Refrigerant | Type | R-134a
Capacity [oz.(g)] | 19.4 ± 0.88 oz. (550 ± 25g)

Blower Unit

Item | Specification
Fresh and recirculation | Operating method | Actuator
Blower | Type | Sirocco
Speed step | Auto + 8 speed (Automatic), 1~4speed (Manual)
Speed control | Power mosfet (Auto) , Resistor (Manual)
Air filter | Type | Particle filter

Heater And Evaporator Unit

Item | Specification
Heater | Type | Pin & Tube type
Heating capacity | 4,850 - 5% kcal/hr
Mode operating method | Actuator
Temperature operating method | Actuator
Evaporator | Temperature control type | Evaporator temperature sensor
A/C ON/OFF [°C(°F)] | ON : 3.0 ± 0.5 (39.4 ± 32.9), OFF: 0 ± 0.5 (32.0 ± 32.9)