| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Lighting System > Rheostat>Repair procedures |

Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Remove the lower crash pad switch (A) from the side crash pad cover by using the scraper. [LHD] [RHD]

3. | Disconnect the rheostat connector (A) from lower crash pad switch.

4. | Operate the rheostat switch and check for continuity between terminals.