| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Button Engine Start System > Start/Stop Button>Repair procedures |

Removal

1. | Disconnect the negative(-) battery terminal.

2. | Remove the crash pad lower panel. (Refer to the BD group - "Crash pad")

3. | Remove the crash pad center lower cover (A) after loosening the mounting screws.

4. | Remove the key set bezel (A) after loosening the mounting screw.

5. | Disconnect the start/stop button connector (A).

6. | Remove the start/stop button (A) by pushing the both sides of the hooks.

Installation

1. | Install the start/stop button.

2. | Install the key set bezel.

3. | Install the crash pad center lower cover.

4. | Install the crash pad lower panel.