| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Sun Roof > Sunroof Switch>Repair procedures |

Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Open the sunglass case cover from the overhead console then remove the 2 screws holding the overhead console (A).

3. | Disconnect the connector. Check for continuity between the terminals. If the continuity is not as specified, replace the sunroof switch.