| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Power Door Mirrors > Power Door Mirror Actuator>Repair procedures |

Inspection

1. | Remove the front door quadrant delta cover. (Refer to the BD group - "Front door")

2. | Disconnect the power door mirror connector from the harness.

3. | Apply battery voltage to each terminal as shown in the table and verify that the mirror operates properly. Mirror Heater Inspection Side Repeater Lamp