| SONATA(YF) >2012 > G 2.4 GDI > Body (Interior and Exterior) > Exterior > Fender>Repair procedures |

Replacement

• | Be careful not to damage the hood and body.

• | Use a clip remover when removing clips.

1. | Remove the front bumper. (Refer to the BD group - "Front Bumper")

2. | Loosen the mud guard mounting screws.

3. | After loosening the mounting screws and clips, then remove the side sill garnish (A).

4. | After loosening the mounting screw and bolt, then remove the front bumper side mounting bracket (A).

5. | After loosening the fender mounting screw and bolts, then remove the fender (A).

6. | Installation is the reverse of removal.