| SONATA(YF) >2013 > G 2.4 GDI > Heating,Ventilation, Air Conditioning > Blower > Climate Control Air Filtar>Repair procedures |

Replacement

1. | Disconnect the damper (B) from the glove box (A).

2. | Disconnect the glove box lift (C).

3. | Remove the filter cover (A) with pushing the knob.

4. | Replace the air filter (B), install it after making sure of the direction of air filter.

In case of driving in an air-polluted area or rugged terrain, check and replace the air filter as frequently as possible.

5. | Installation is the reverse order of removal.