| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Lighting System > Rear combination lamp>Repair procedures |

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove the rear combination lamp cover (A).

3. | Remove the rear combination lamp after loosening the mounting nuts (4EA) and disconnecting the connector (A).

4. | If necessary to remove the bulb, remove the bulb after removing rear combination cover. [Tail Lamp / Stop Lamp] [Turn Signal Lamp] [Tail Lamp]

5. | Remove the trunk lid trim. (Refer to the BD group - "Trunk")

6. | Remove the trunk lid lamp assembly (A) after loosening the mounting nuts (3EA) and disconnecting the connector.

7. | Replace the bulb after removing the trunk lid lamp assembly. [Tail Lamp] [Back Up Lamp]

Installation

1. | Install the trunk lid lamp assembly.

2. | Install the rear combination lamp.