| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Multifunction switch>Specifications |

Specifications

Items | Specifications
Rated voltage | DC 12V
Operating temperature range | -30°C ~ +80°C (-22 ~ +176°F)
Rated load | Dimmer & passing switch | High : 1.0A (Relay load) Low : 1.0A (Relay load) Passing : 1.0A (Relay load)
Lighting switch | Lighting : 1.0A (Relay load)
Turn signal & lane change switch | 6.6 ± 0.5A (Lamp load)
Front & rear fog lamp switch | 1.0A (Relay load)
Wiper & mist switch | Low, High : 4.0A (Motor load) Intermittent : 0.22 ± 0.05A (Relay load) Lock : Max. 28A (Motor load)
Washer switch | 4A (Motor load)
Variable intermittent volume switch | Max. 25mA