| SONATA(YF) >2012 > G 2.4 GDI > Body (Interior and Exterior) > Bumper > Rear Bumper>Repair procedures |

Replacement

• | After remove the rear combination lamp.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts your hands.

• | Put on gloves to protect your hands.

• | Take care not bend or scratch the cover and other parts.

1. | Remove the following items.

A. | Luggage cover mat (Refer to the BD group - "Trunk Trim")

B. | Transverse trim (Refer to the BD group - "Trunk Trim")

C. | Luggage side trim (Refer to the BD group - "Trunk Trim")

2. | Remove the rear combination lamp cover (A).

3. | Disconnect the connector (A), and then remove the rear combination lamp mounting nuts.

4. | Remove the rear combination lamp.

5. | After loosening the rear bumper side's mounting clip and screws, then disconnect the side's.

6. | Remove the mounting bolts.

7. | Disconnect the connector (A).

8. | Loosen the rear bumper cover mounting clips, and then remove the rear bumper cover (A).

9. | Installation is the reverse of removal.

• | Replace any damage clips.