| SONATA(YF) >2013 > G 2.4 GDI > Restraint > Airbag Module > Curtain Airbag (CAB) Module>Repair procedures |

Removal

1. | Disconnect the battery negative cable and wait for at least 3 minutes before beginning work.

2. | Remove the roof trim. (Refer to the Body group- Interior)

3. | Disconnect the curtain airbag harness connector.

4. | After loosening the mounting bolts and nuts remove the curtain airbag.

Installation

1. | Remove the ignition key from the vehicle.

2. | Disconnect the battery negative cable and wait for at least three minutes.

3. | Tighten the curtain airbag mounting bolts and nuts.

Tightening torque:
Bolts : 9.8 ~ 14.7 N.m (1.0 ~ 1.5 kgf.m, 7.2 ~ 10.8 lb-ft)
Nuts : 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)

• | Never twist the airbag module during installation. If the airbag module is twisted, it may not operate as designed.

4. | Connect the curtain airbag connector.

5. | Install the roof trim. (Refer to the Body group- Interior)

6. | Reconnect the battery negative cable.

7. | After installing the curtain airbag (CAB), confirm proper system operation:

A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.