| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > MTS System > MTS Antenna>Repair procedures |

Removal

Roof Antenna (GPS)

1. | Remove the rear roof trim. (Refer to the BD group - "Roof trim")

2. | Disconnect the GPS (A) cable from the roof antenna.

3. | Remove the roof antenna (A) after removing a nut

Installation

Roof Antenna (GPS)

1. | Installation the roof antenna.

2. | Connect the GPS cable.

3. | Install the rear roof trim.

- | Make sure that the cables and connectors are plugged in properly.

- | Check the AVN system.