| SONATA(YF) >2012 > G 2.4 GDI > Body (Interior and Exterior) > Seat & Power Seat > Rear Seat>Repair procedures |

Replacement

Seat Assembly Replacement

1. | After loosening the mounting bolts, then remove the rear seat assembly (A).

Tightening torque :
44.1 ~ 58.8 N.m (4.5 ~ 6.0 kgf.m, 32.5 ~ 43.4 lb-ft)

2. | Disconnect the seat heater connectors (A).

3. | Installation is the reverse of removal.

Seat mounting bolt and nut installation procedure.

• | Tighten temporarily in the order of nut and bolt on the front of recliner hinge installation part.

• | After completely tightening completely the bolt on the back of the recliner hinge installaion part, tighten the bolt on the front of it completely.

• | Setting down the seat cushion, tighten the mounting bolt of the cushion frame hinge.

• | Check if reclining the seat and folding seat back operate smoothly.

Armrest Replacement

1. | After loosening the mounting nuts, then remove the armrest(A).

2. | Installation is the reverse of removal.