| SONATA(YF) >2012 > G 2.4 GDI > Automatic Transaxle System > Automatic Transaxle Control System > Inhibiter Switch>Repair procedures |

Removal

1. | Set room side lever and T/M side lever to "N" position.

2. | Remove the battery and the battery tray. (Refer to "Charging system" in EE group.)

3. | Remove the air cleaner assembly. (Refer to "Intake manifold" in EM group.)

4. | Remove the shift cable mounting nut (B).

5. | Disconnect the inhibitor switch connector (A).

6. | Remove the manual control lever (A) and the washer (B) after removing a nut (C).

When installing, fix the manual control lever and the inhibitor switch with Ø5mm (0.1969in.) fixing jig.
And then tighten the inhibitor assembly mounting bolts.

7. | Remove the inhibitor assembly (A) after removing the bolts (2ea).

Tightening torque:
9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)

When installing, tighten the inhibitor assembly mounting bolt lightly.

Installation

1. | Installation is the reverse of removal.