| SONATA(YF) >2013 > G 2.4 GDI > Heating,Ventilation, Air Conditioning > Controller > Heater & A/C Control Unit(Manual)>Repair procedures |

Replacement

1. | Disconnect the negative (-) battery terminal.

2. | Remove the crash pad garnish (A).

3. | Using the screwdriver, remove the center facia panel (A).

4. | Disconnect the connectors (A) and then remove the center facia panel from the crash pad.

5. | Remove the heater and A/C controller (A) from the center facia.

6. | Installation is the reverse order of removal.