| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Windshield Deicer > Windshield Deicer>Repair procedures |

Inspection

1. | Remove the cowl top cover. (Refer to the wiper)

2. | Disconnect the windshield deicer connector (A) from the wiper motor linkage.

3. | Check for continuity between the terminals of deicer lines.

4. | Turn the ignition switch ON and the windshield deicer switch ON, then measure the voltage between the terminals of harness side deicer connector.

OK : approx. Battery voltage