| SONATA(YF) >2013 > G 2.4 GDI > Engine Control/Fuel System > Fuel Delivery System > Fuel Pump>Repair procedures |

Removal

1. | Release the residual pressure in fuel line (Refer to “Release Residual Pressure in Fuel Line” in this group).

2. | Remove the fuel pump service cover (A) in the trunk.

3. | Disconnect the fuel pump connector (A) and the fuel tank pressure sensor connector (B).

4. | Disconnect the fuel feed tube quick connector (C) and the vapor tube quick-connector (D).

5. | Remove locking ring (E) by use the special service tool [SST No. : 09310-2S200].

6. | Disconnector the vapor tube quck-connector (A) at the fuel pump, and then remove the fuel pump from the fuel tank.

Installation

1. | Installation is reverse of removal.

Be careful of fuel pump direction (Refer to the groove in the fuel tank).