| SONATA(YF) >2012 > G 2.4 GDI > Manual Transaxle System > General Information>Specifications |

Specifications

Manual transaxle type | M6GF2
Engine type | Gasoline 2.4 GDI
Gear ratio | 1st | 3.267
2nd | 1.931
3rd | 1.696
4th | 1.276
5th | 1.027
6th | 0.829
Reverse | 3.588
Final gear ratio | 4.333(1,2,R)/ 3.250(3~6)

Tightening Torques

Item | N.m | kgf.m | lb-ft
Oil drain plug | 58.9 ~ 78.5 | 6.0 ~ 8.0 | 43.4 ~ 57.9
Oil filler plug | 29.4 ~ 34.3 | 3.0 ~ 3.5 | 21.7 ~ 25.3
Shift lever assembly | 8.8 ~ 13.7 | 0.9 ~ 1.4 | 6.5 ~ 10.1
Back up lamp switch | 29.4 ~ 34.3 | 3.0 ~ 3.5 | 21.7 ~ 25.3
Starter motor mounting bolt | 42.2 ~ 53.9 | 4.3 ~ 5.5 | 31.1 ~ 39.8
Transaxle mounting support bracket bolt | 68.7 ~ 93.2 | 7.0 ~ 9.5 | 50.6 ~ 68.7
Manual transaxle upper mounting bolt | 42.2 ~ 53.9 | 4.3 ~ 5.5 | 31.1 ~ 39.8
Manual transaxle lower mounting bolt | (A) 42.2 ~ 48.1 (B) 42.2 ~ 53.9 | 4.3 ~ 4.9 4.3 ~ 5.5 | 31.1 ~ 35.5 31.1 ~ 39.8

Lubricants

Items | Recommended lubricant | Quantity
Transaxle gear oil | SAE 75W/85 API GL-4 | 1.8L(0.48 U.S.gal., 1.90 U.S. qt., 1.58 lmp.qt.)