| SONATA(YF) >2012 > G 2.4 GDI > Engine Electrical System > General Information>Specifications |

Specifications

Ignition System

Items | Specifications
Ignition coil | Primary resistance | 0.62 ± 10 % (Ω)
Secondary resistance | 7.0 ± 15 % (kΩ)
Spark plugs | Type | FXU16HR11
Gap | 1.0 ~ 1.1 mm (0.0394 ~ 0.0433 in.)

Starting System

Items | Specifications
REMY | VALEO
Starter | Rated voltage | 12V, 1.2kW
No. of pinion teeth | 11
No-load characteristics | Voltage | 11.5V | 11V
Ampere | 105A, MAX | 70A, MAX
Speed | 2,950rpm, MIN | 2,400rpm, MIN

Charging System

Items | Specifications
Alternator | Type | Battery voltage sensing
Rate voltage | 13.5 V, 110A
Speed in use | 1,000 ~ 18,000 rpm
Voltage regulator | IC regulator built-in type
Regulator setting voltage | External mode | ECU control
Internal mode | 14.1 ± 0.3V
Temperature compensation | External mode | ECU control
Internal mode | -3.5 ± 2mV / °C
Battery | Type | 54-26GL
Cold cranking amperage [at -18°C(-0.4°F)] | 600A
Reserve capacity | 110min
Specific gravity [at 25°C(77°F)] | 1.280 ± 0.01

• | COLD CRANKING AMPERAGE is the amperage a battery can deliver for 30 seconds and maintain a terminal voltage of 7.2V or greater at a specified temperature.

• | RESERVE CAPACITY RATING is amount of time a battery can deliver 25A and maintain a minimum terminal voltage of 10.5V at 26.7°C(80.1°F).