| SONATA(YF) >2012 > G 2.4 GDI > Engine Control/Fuel System > Engine Control System > Purge Control Solenoid Valve (PCSV)>Repair procedures |

Inspection

1. | Turn the ignition switch OFF.

2. | Disconnect the PCSV connector.

3. | Measure resistance between the PCSV terminals 1 and 2.

4. | Check that the resistance is within the specification.

Specification: Refer to “Specification”

Removal

1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.

2. | Disconnect the purge control solenoid valve connector (A).

3. | Disconnect the vapor hoses (B) from the purge control solenoid valve.

4. | Remove the valve from the bracket (C) in the direction of the arrow.

Installation

• | Install the component with the specified torques.

• | Note that internal damage may occur when the component is dropped. If the component has been dropped, inspect before installing.

• | Use care to keep foreign material out of the valve.

1. | Installation is reverse of removal.

Purge control solenoid valve bracket installation bolt: 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)