| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Immobilizer System > Antenna Coil>Repair procedures |

Replacement

1. | Disconnect the negative (-) battery terminal.

2. | Remove the steering column upper and lower shrouds after loosening the screws (3EA).

3. | Disconnect the 6P connector (B) of the coil antenna and then remove the coil antenna (A) after loosening the screw.

4. | Installation is the reverse of removal procedure.