| SONATA(YF) >2012 > G 2.4 GDI > Body (Interior and Exterior) > Interior > Trunk Trim>Repair procedures |

Replacement

• | Put on gloves to protect your hands.

• | When plying with a flat-tip screwd river, wrap it with protective tape to prevent damage.

• | Take care not to bend or scratch the trim and panels.

1. | Remove the trunk trim.

2. | Installation is the reverse of removal.

• | Replace any damage clips.

1. Luggage side trim 2. Rear transverse trim 3. Board & jack handle assembly | 4. Luggage cover met 5. Luggage side board (LH) 6. Luggage side tray (RH)