| SONATA(YF) >2012 > G 2.4 GDI > Emission Control System > General Information>Specifications |

Specifications

Purge Control Solenoid Valve (PCSV)
▷ Specification

Item | Specification
Coil Resistance (Ω) | 19.0 ~ 22.0 [20°C(68°F)]

Fuel Tank Pressure Sensor (FTPS)
▷ Type: Piezo-Resistive Pressure Sensor
▷ Specification

Pressure [kPa (kgf/cm², in H2O)] | Output Voltage (V)
-6.67 (-0.068, -26.8) | 0.5
0 | 2.5
+6.67 (0.068, 26.8) | 4.5

Canister Close Valve (CCV)
▷ Specification

Item | Specification
Coil Resistance (Ω) | 19.9 ~ 22.9 [20°C(68°F)]

Tightening Torques

Item | kgf.m | N.m | lb-ft
Positive crankcase ventilation valve installation | 0.19 ~ 0.29 | 1.9 ~ 2.8 | 1.4 ~ 2.1
Canister installation bolt | 0.4 ~ 0.6 | 3.9 ~ 5.9 | 2.9 ~ 4.3