| SONATA(YF) >2013 > G 2.4 GDI > Heating,Ventilation, Air Conditioning > Air Conditioning System > Condenser>Repair procedures |

Inspection

1. | Check the condenser fins for clogging and damage. If clogged, clean them with water, and blow them with compressed air. If bent, gently bend them using a screwdriver or pliers.

2. | Check the condenser connections for leakage, and repair or replace it, if required.

Replacement

1. | Recover the refrigerant with a recovery/ recycling/ charging station.

2. | Disconnect the negative (-) battery terminal.

3. | Remove the discharge line and liquid line (A) from the condenser.

4. | Remove the front bumper upper cover (A).

5. | Remove the intake air filter cover (A).

6. | Remove the front bumper frame (A).

7. | Remove the condenser (A) from radiator.

8. | Install in the reverse order of removal, and note these items :

- | If you're installing a new condenser, add refrigerant oil ND-OIL8.

- | Replace the O-rings with new ones at each fitting, and apply a thin coat of refrigerant oil before installing them. Be sure to use the right O-rings for R-134a to avoid leakage.

- | Be careful not to damage the radiator and condenser fins when installing the condenser.

- | Be sure to install the lower mount cushions of condenser securely into the holes.

- | Charge the system, and test its performance.