| SONATA(YF) >2012 > G 2.4 GDI > Brake System > Brake System > Brake Line>Repair procedures |

Removal

1. | Disconnect the brake fiuid level switch connector, and remove the reservoir cap.

2. | Remove the brake fluid from the master cylinder reservior with a syringe.

Do not spill brake fluid on the vehicle, it may damage the paint; if brake fluid does contact the paint, wash it off immediately with water.

3. | Remove the wheel & tire.

4. | Remove the brake hose clip (A). Front Rear

5. | Disconnect the brake tube by loosening the tube flare nut (B).

Tightening torque:
13.7 ~ 16.7N.m (1.4 ~ 1.7kgf.m, 10.1 ~ 12.3lb-ft)

6. | Disconnect the brake hose from the brake caliper by loosening the bolt (C).

Tightening torque:
24.5 ~29.4 N.m (2.5 ~3.0 kgf.m, 18.1 ~21.7 lb-ft)

Front

Rear

Inspection

1. | Check the brake tubes for cracks, crimps and corrosion.

2. | Check the brake hoses for cracks, damage and fluid leakage.

3. | Check the brake tube flare nuts for damage and fluid leakage.

4. | Check brake hose mounting bracket for crack or deformation.

Installation

1. | Installation is the reverse of removal.

Use a new washer (A) whenever installing.

2. | After installation, bleed the brake system. (Refer to Brake system bleeding)

3. | Check the spilled brake oil.