| SONATA(YF) >2012 > G 2.4 GDI > Heating,Ventilation, Air Conditioning > Blower > Blower Unit>Repair procedures |

Replacement

1. | Disconnect the negative (-) battery terminal.

2. | Remove the crash pad. (Refer to BD group - "Crash Pad")

3. | Remove the cowl cross bar assembly. (Refer to BD group - "Crash Pad")

4. | Remove the heater and blower unit. (Refer to HA group - "Heater Unit")

5. | Remove the blower unit (A) from the heater unit after loosening a mounting bolt and 3 screws.

Make sure that there is no air leaking out of the blower and duct joints.

6. | Installation is the reverse order of removal.