| SONATA(YF) >2012 > G 2.4 GDI > Restraint > SRSCM>Schematic Diagrams |

Circuit Diagram (1)

Circuit Diagram (2)

Circuit Diagram (3)

SRSCM Connector Terminal

Pin | Function (Connector A) | Pin | Function (Connector A)
1 | Ignition | 1 | Side impact sensor [Passenger] High
2 | - | 2 | Side impact sensor [Passenger] Low
3 | - | 3 | Side impact sensor [Driver] High
4 | Front impact sensor [Driver] High | 4 | Side impact sensor [Driver] Low
5 | Front impact sensor [Driver] Low | 5 | Pressure side impact sensor [Passenger] High
6 | Front impact sensor [Passenger] High | 6 | Pressure side impact sensor [Passenger] Low
7 | Front impact sensor [Passenger] Low | 7 | Pressure side impact sensor [Driver] High
8 | CAN_Low | 8 | Pressure side impact sensor [Driver] Low
9 | CAN_High | 9 | Ground
10 | Shorting bar | 10 | -
11 | Shorting bar | 11 | -
12 | (1st stage) Driver airbag High | 12 | Seat belt buckle switch [Driver] High
13 | (1st stage) Driver airbag Low | 13 | Seat belt buckle switch [Driver] Low
14 | (1st stage) Passenger airbag Low | 14 | Seat belt pretensioner [Driver] High
15 | (1st stage) Passenger airbag High | 15 | Seat belt pretensioner [Driver] Low
16 | - | 16 | Seat belt pretensioner [passenger] Low
17 | - | 17 | Seat belt pretensioner [passenger] High
18 | - | 18 | Curtain airbag [Driver] High
19 | - | 19 | Curtain airbag [Driver] Low
20 | - | 20 | -
21 | Seat belt reminder | 21 | -
22 | Crash Output | 22 | -
23 | (2nd stage) Driver airbag Low | 23 | -
24 | (2nd stage) Driver airbag High | 24 | -
25 | (2nd stage) Passenger airbag High | 25 | Seat belt buckle swich [Passenger] High
26 | (2nd stage) Passenger airbag Low | 26 | Seat belt buckle swich [Passenger] Low
27 | Telltale Indicator | 27 | Side airbag [Driver] High
|  | 28 | Side airbag [Driver] Low
|  | 29 | Side airbag [Passenger] Low
|  | 30 | Side airbag [Passenger] High
|  | 31 | Curtain airbag [Passenger] High
|  | 32 | Curtain airbag [Passenger] Low
|  | 33 | Anchor Pretensioner [Driver] Low
|  | 34 | Anchor Pretensioner [Driver] High
|  | 35 | Anchor Pretensioner [Passenger] High
|  | 36 | Anchor Pretensioner [Passenger] Low
|  | 37 | -
|  | 38 | Seat track position sensor [Driver] High
|  | 39 | Seat track position sensor [Driver] Low