| SONATA(YF) >2013 > G 2.4 GDI > Manual Transaxle System > Manual Transaxle Control System > Shift Lever>Repair procedures |

Removal

1. | Remove the front console assembly.(Refer to "Interior" in BD group)

2. | Remove the snap pin (A) and the clips (B).

3. | Remove the clip(A) from the shift cable.

4. | Remove the shift lever assembly (A).

Tightening torque :
8.8~13.7N.m (0.9~1.4kgf.m, 6.5~10.1Ib-ft)

5. | Remove the retainer (A) and the nuts (B).

Tightening torque :
9.8~14.7N.m (1.0~1.5kgf.m, 7.2~10.8Ib-ft)

6. | Remove the cable from the bracket at tranmission side (Refer to "Transaxle" in this group).

7. | Remove the select cable and shift cable.

Inspection

1. | Check the select cable for proper operation and for damage.

2. | Check the shift cable for proper operation and for damage.

3. | Check the boots for damage.

4. | Check the boots for wear abrasion sticking, restricted movement or damage.

5. | Check for the weak or damaged spring.

Installation

1. | Installation is the reverse of removal.

• | Move the slide clip (B) of guide member (A) in the direction as shown in the illustration. Adjust the slide clip fit into the select lever moving the slide clip in the direction(C).

• | Install the guide member (A) of the select cable (B).

• | Adjust the slide clip (B) to fit it into the select lever pin (A) and install the snap pin (C). Insert the slide clip in the direction as shown in the illustration.