| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Indicators And Gauges>Troubleshooting |

Troubleshooting

Symptom | Possible cause | Remedy
Speedometer does not operate | Fuse (MODULE1 7.5A and Room lamp 10A) in smart junction box is blown | Check for short and replace fuse
Speedometer faulty | Check speedometer
Vehicle speed sensor faulty | Check vehicle speed sensor
Wiring or ground faulty | Repair if necessary
Tachometer does not operate | Fuse (MODULE1 7.5A and Room lamp 10A) in smart junction box is blown | Check for short and replace fuse
Tachometer faulty | Check tachometer
Wiring or ground faulty | Repair if necessary
Fuel gauge does not operate | Fuse (MODULE1 7.5A and Room lamp 10A) in smart junction box is blown | Check for short and replace fuse
Fuel gauge faulty | Check gauge
Fuel sender faulty | Check fuel sender
Wiring or ground faulty | Repair if necessary
Low fuel warning lamp does not light up | MODULE1 7.5A fuse in smart junction box is blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Fuel sender faulty | Check fuel sender
Wiring or ground faulty | Repair if necessary
Water temperature gauge does not operate | MODULE1 7.5A fuse in smart junction box is blown | Check for short and replace fuse
Water temperature gauge faulty | Check gauge
Water temperature sender faulty | Check sender
Wiring or ground faulty | Repair if necessary
Oil pressure warning lamp does not light up | MODULE1 7.5A fuse in smart junction box is blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Oil pressure switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Parking brake warning lamp does not light up | MODULE1 7.5A fuse in smart junction box is blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Brake fluid level warning switch faulty | Check switch
Parking brake switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Open door warning lamp and trunk lid warning lamp do not light up | Room lamp 10A fuse in smart junction box is blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Door switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Seat belt warning lamp does not light up | MODULE1 7.5A fuse in smart junction box is blown | Check for short and replace fuse
Bulb burned out | Replace bulb
Seat belt switch faulty | Check switch
Wiring or ground faulty | Repair if necessary