| SONATA(YF) >2013 > G 2.4 GDI > Emission Control System > Evaporative Emission Control System > Fuel Tank Air Filter>Repair procedures |

Removal

1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.

2. | Disconnect the canister close valve connector (A).

3. | Disconnect the ventilation tube quick connector (B).

4. | Release the lever (C), and then remove the fuel tank air filter (D) after rotating it in the direction of the arrow in the figure.

Installation

• | Install the component with the specified torques.

• | Note that internal damage may occur when the component is dropped. In this case, use it after inspecting.

1. | Installation is reverse of removal.