| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Power Door Mirrors > Power Out Side Mirror Switch>Repair procedures |

Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Remove the front door trim panel. (Refer to the BD group - "Front door")

3. | Disconnect the connector from the power window switch module.

4. | Check for continuity between the terminals in each switch position according to the table. [Power Mirror Switch]