| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Lighting System > Front Fog Lamps>Repair procedures |

Inspection

1. | Disconnect the negative(-) battery terminal.

2. | Remove the lighting switch of the multi-function switch. (Refer to the multi-function switch)

3. | With the front fog lamp switch, make sure that continuity exists between the terminals below. If continuity is not as specified, replace the multi-function switch. Front Fog Lamp

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove the front bumper. (Refer to the BD group - "Front bumper")

3. | Disconnect the front fog lamp connector (A).

4. | Replace the front fog bulb (A) turning it in the counter clock-wise direction.

Installation

1. | Install the front fog bulb.

2. | Reconnect the lamp connector.

3. | Install the front bumper.