| SONATA(YF) >2013 > G 2.4 GDI > Heating,Ventilation, Air Conditioning > Blower > Blower Resistor>Repair procedures |

Inspection

1. | Measure terminal - to - terminal resistance of blower resistor.

2. | If measure resistance isnot within specification, the blower resistor must be replaced.

Replacement

1. | Disconnect the negative (-) battery terminal.

2. | Remove the crash pad lower panel (A).

3. | Disconnect the blower resistor connector (A) and then remove the blower resistor (B) after loosening the mounting screws.

4. | Installation is the reverse order of removal.