| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Seat Electrical > Seat Heater Switch>Repair procedures |

Inspection

Front Seat Heater Switch

1. | Disconnect the negative (-) battery terminal.

2. | Remove the floor console upper cover (A).

3. | Disconnect the multimedia jack connector (A) from the floor console upper cover.

4. | Remove the seat heater switch connectors from the floor console upper cover (A).

5. | Operate each seat heater switch and check that continuity exists between the terminals. If there is no continuity, replace the seat heater switch

Rear Seat Heater Switch

1. | Disconnect the negative (-) battery terminal.

2. | Remove the rear door trim. (Refer to the BD group - "Rear door")

3. | Turn rear seat heater switch ON and check that continuity exists between the terminals. If there is no continuity, replace the seat heater switch.

Installation

1. | Install the seat heater switch.

2. | Install the console upper cover.

3. | Install the shift lever knob.