| SONATA(YF) >2013 > G 2.4 GDI > Suspension System > Rear Suspension System > Trailing Arm>Repair procedures |

Replacement

1. | Remove the rear wheel & tire.

Tightening torque:
88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft)

Be careful not to damage to the hub bolts when removing the rear wheel & tire.

2. | Disconnect the parking brake cable (A) with the rear brake assembly.

3. | Loosen the parking brake cable bracket nuts (A) & trailing arm mounting nuts (B) and then remove the trailing arm with the rear axle.

Tightening torque:
44.1 ~ 53.9 N.m (4.5 ~ 5.5 kgf.m, 32.5 ~ 39.8 lb-ft)

4. | Loosen the parking brake cable bracket bolt (A).

5. | Loosen the mounting bolt and then remove the trailing arm (A) with the frame.

Tightening torque:
98.1 ~ 117.7 N.m (10.0 ~ 12.0 kgf.m, 72.3 ~ 86.8 lb-ft)

6. | Installation is the reverse of removal.