| SONATA(YF) >2012 > G 2.4 GDI > Body (Interior and Exterior) > Exterior > Mirror>Repair procedures |

Replacement

Outside Rear View Mirror Replacement

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.

• | Put on gloves to protect your hands.

1. | Using a screwdriver, remove the quadrant inner cover (A).

2. | After disconnecting the connector (A), remove the outside rear view mirror (B).

Tightening torque :
6.9~10.8 N.m(0.7~1.1 kgf.m, 5.1~8.0 lb-ft)

3. | Installation is the reverse of removal.

Inside Rear View Mirror Assembly Replacement

ECM Mirror Replacement

1. | Remove the ECM mirror cover (A).

2. | After loosening the mounting screw (A), then disconnect the connector (B).

3. | Push the ECM mirror base up to remove the ECM mirror assembly (A).

4. | Installation is the reverse of removal.