| SONATA(YF) >2013 > G 2.4 GDI > Engine Control/Fuel System > Engine Control System > CVVT Oil Control Valve (OCV)>Repair procedures |

Inspection

1. | Turn the ignition switch OFF.

2. | Disconnect the OCV connector.

3. | Measure resistance between the OCV terminals 1 and 2.

4. | Check that the resistance is within the specification.

Specification: Refer to “Specification”

Removal

1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.

2. | Disconnect the CVVT oil control valve connector (A).

3. | Remove the installation bolt (B), and then remove the valve from the engine. [Bank 1 / Intake] [Bank 1 / Exhaust]

Installation

• | Install the component with the specified torques.

• | Note that internal damage may occur when the component is dropped. If the component has been dropped, inspect before installing.

• | Apply engine oil to the valve O-ring.

1. | Installation is reverse of removal.

CVVT oil control valve installation bolt:
9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)